**Park Quadrant door handle tightening instructions**

****

1. Unscrew grub screw in each handle with an allen key

A picture containing indoor, bicycle, steel, aluminium

Description automatically generated



1. Unscrew the rings covering the base of each handle by turning



1. Unscrew the two screws attaching bolts through door with flat headed screwdriver

A picture containing floor, indoor, silver

Description automatically generated



1. Unscrew the small screw at the top, holding on the handle at side to be tightened



1. Remove the handle to be tightened
2. Tighten the handle using an allen key placed down the centre

A close up of a tool

Description automatically generated with low confidence

1. Replace parts in reverse order from steps 6 to 1 above.